[6:14:24 PM]:3    COM3     5.004978s     resdump:<?xml version="1.0" encoding="UTF-8" ?>
<data>
<log value="ERROR: Only nop and sig tag can be recevied before authentication." /></data><?xml version="1.0" encoding="UTF-8" ?>
<data>
<response value="NAK" rawmode="false" /></data>


[6:15:40 PM]:3    COM3     80.0859144s     System.Exception: authentication failed Cannot create a file when that file already exists
   at XiaoMiFlash.code.bl.SerialPortDevice.dlAuth()
   at XiaoMiFlash.code.bl.SerialPortDevice.ConfigureDDR(Int32 intSectorSize, Int32 buffer_sectors, String ddrType, Int32 m_iSkipStorageInit)
   at XiaoMiFlash.code.bl.SerialPortDevice.XiaomiFlashNew()     at XiaoMiFlash.code.bl.SerialPortDevice.dlAuth()
   at XiaoMiFlash.code.bl.SerialPortDevice.ConfigureDDR(Int32 intSectorSize, Int32 buffer_sectors, String ddrType, Int32 m_iSkipStorageInit)
   at XiaoMiFlash.code.bl.SerialPortDevice.XiaomiFlashNew()
[6:20:14 PM]:3    COM3     5.0212689s     resdump:<?xml version="1.0" encoding="UTF-8" ?>
<data>
<log value="ERROR: Only nop and sig tag can be recevied before authentication." /></data><?xml version="1.0" encoding="UTF-8" ?>
<data>
<response value="NAK" rawmode="false" /></data>


[6:20:44 PM]:3    COM3     35.0324826s     System.Exception: authentication failed Cannot create a file when that file already exists
   at XiaoMiFlash.code.bl.SerialPortDevice.dlAuth()
   at XiaoMiFlash.code.bl.SerialPortDevice.ConfigureDDR(Int32 intSectorSize, Int32 buffer_sectors, String ddrType, Int32 m_iSkipStorageInit)
   at XiaoMiFlash.code.bl.SerialPortDevice.XiaomiFlashNew()     at XiaoMiFlash.code.bl.SerialPortDevice.dlAuth()
   at XiaoMiFlash.code.bl.SerialPortDevice.ConfigureDDR(Int32 intSectorSize, Int32 buffer_sectors, String ddrType, Int32 m_iSkipStorageInit)
   at XiaoMiFlash.code.bl.SerialPortDevice.XiaomiFlashNew()
[6:31:48 PM]:1    6cf060e4     5.0244024s     can not found file flash_all_lock.bat
[6:32:22 PM]:3    COM3     5.026109s     resdump:<?xml version="1.0" encoding="UTF-8" ?>
<data>
<log value="ERROR: Only nop and sig tag can be recevied before authentication." /></data><?xml version="1.0" encoding="UTF-8" ?>
<data>
<response value="NAK" rawmode="false" /></data>


[6:32:52 PM]:3    COM3     35.0429877s     System.Exception: authentication failed Cannot create a file when that file already exists
   at XiaoMiFlash.code.bl.SerialPortDevice.dlAuth()
   at XiaoMiFlash.code.bl.SerialPortDevice.ConfigureDDR(Int32 intSectorSize, Int32 buffer_sectors, String ddrType, Int32 m_iSkipStorageInit)
   at XiaoMiFlash.code.bl.SerialPortDevice.XiaomiFlashNew()     at XiaoMiFlash.code.bl.SerialPortDevice.dlAuth()
   at XiaoMiFlash.code.bl.SerialPortDevice.ConfigureDDR(Int32 intSectorSize, Int32 buffer_sectors, String ddrType, Int32 m_iSkipStorageInit)
   at XiaoMiFlash.code.bl.SerialPortDevice.XiaomiFlashNew()
[6:35:03 PM]:3    COM3     5.0006219s     resdump:<?xml version="1.0" encoding="UTF-8" ?>
<data>
<log value="ERROR: Only nop and sig tag can be recevied before authentication." /></data><?xml version="1.0" encoding="UTF-8" ?>
<data>
<response value="NAK" rawmode="false" /></data>


[6:35:33 PM]:3    COM3     35.0715665s     System.Exception: authentication failed Cannot create a file when that file already exists
   at XiaoMiFlash.code.bl.SerialPortDevice.dlAuth()
   at XiaoMiFlash.code.bl.SerialPortDevice.ConfigureDDR(Int32 intSectorSize, Int32 buffer_sectors, String ddrType, Int32 m_iSkipStorageInit)
   at XiaoMiFlash.code.bl.SerialPortDevice.XiaomiFlashNew()     at XiaoMiFlash.code.bl.SerialPortDevice.dlAuth()
   at XiaoMiFlash.code.bl.SerialPortDevice.ConfigureDDR(Int32 intSectorSize, Int32 buffer_sectors, String ddrType, Int32 m_iSkipStorageInit)
   at XiaoMiFlash.code.bl.SerialPortDevice.XiaomiFlashNew()
[6:37:26 PM]:3    COM3     5.01659s     resdump:<?xml version="1.0" encoding="UTF-8" ?>
<data>
<log value="ERROR: Only nop and sig tag can be recevied before authentication." /></data><?xml version="1.0" encoding="UTF-8" ?>
<data>
<response value="NAK" rawmode="false" /></data>


[6:37:56 PM]:3    COM3     35.0738726s     System.Exception: authentication failed Cannot create a file when that file already exists
   at XiaoMiFlash.code.bl.SerialPortDevice.dlAuth()
   at XiaoMiFlash.code.bl.SerialPortDevice.ConfigureDDR(Int32 intSectorSize, Int32 buffer_sectors, String ddrType, Int32 m_iSkipStorageInit)
   at XiaoMiFlash.code.bl.SerialPortDevice.XiaomiFlashNew()     at XiaoMiFlash.code.bl.SerialPortDevice.dlAuth()
   at XiaoMiFlash.code.bl.SerialPortDevice.ConfigureDDR(Int32 intSectorSize, Int32 buffer_sectors, String ddrType, Int32 m_iSkipStorageInit)
   at XiaoMiFlash.code.bl.SerialPortDevice.XiaomiFlashNew()
[6:41:44 PM]:3    COM3     5.021338s     resdump:<?xml version="1.0" encoding="UTF-8" ?>
<data>
<log value="ERROR: Only nop and sig tag can be recevied before authentication." /></data><?xml version="1.0" encoding="UTF-8" ?>
<data>
<response value="NAK" rawmode="false" /></data>


[6:42:14 PM]:3    COM3     35.0789132s     System.Exception: authentication failed Cannot create a file when that file already exists
   at XiaoMiFlash.code.bl.SerialPortDevice.dlAuth()
   at XiaoMiFlash.code.bl.SerialPortDevice.ConfigureDDR(Int32 intSectorSize, Int32 buffer_sectors, String ddrType, Int32 m_iSkipStorageInit)
   at XiaoMiFlash.code.bl.SerialPortDevice.XiaomiFlashNew()     at XiaoMiFlash.code.bl.SerialPortDevice.dlAuth()
   at XiaoMiFlash.code.bl.SerialPortDevice.ConfigureDDR(Int32 intSectorSize, Int32 buffer_sectors, String ddrType, Int32 m_iSkipStorageInit)
   at XiaoMiFlash.code.bl.SerialPortDevice.XiaomiFlashNew()
[6:44:44 PM]:3    COM3     5.0086559s     resdump:<?xml version="1.0" encoding="UTF-8" ?>
<data>
<log value="ERROR: Only nop and sig tag can be recevied before authentication." /></data><?xml version="1.0" encoding="UTF-8" ?>
<data>
<response value="NAK" rawmode="false" /></data>


[6:45:09 PM]:3    COM3     30.0438803s     authentication failed result by Ko Nine
[6:46:36 PM]:3    COM3     20.0240019s     write time out,maybe device was disconnected.
[6:46:46 PM]:3    COM3     0.2722067s     System.IO.IOException: The requested resource is in use.

   at System.IO.Ports.InternalResources.WinIOError(Int32 errorCode, String str)
   at System.IO.Ports.InternalResources.WinIOError(String str)
   at System.IO.Ports.SerialStream..ctor(String portName, Int32 baudRate, Parity parity, Int32 dataBits, StopBits stopBits, Int32 readTimeout, Int32 writeTimeout, Handshake handshake, Boolean dtrEnable, Boolean rtsEnable, Boolean discardNull, Byte parityReplace)
   at System.IO.Ports.SerialPort.Open()
   at XiaoMiFlash.code.bl.SerialPortDevice.registerPort(SerialPort port)     at System.IO.Ports.InternalResources.WinIOError(Int32 errorCode, String str)
   at System.IO.Ports.InternalResources.WinIOError(String str)
   at System.IO.Ports.SerialStream..ctor(String portName, Int32 baudRate, Parity parity, Int32 dataBits, StopBits stopBits, Int32 readTimeout, Int32 writeTimeout, Handshake handshake, Boolean dtrEnable, Boolean rtsEnable, Boolean discardNull, Byte parityReplace)
   at System.IO.Ports.SerialPort.Open()
   at XiaoMiFlash.code.bl.SerialPortDevice.registerPort(SerialPort port)
[6:47:08 PM]:3    COM3     10.0205597s     cannot receive hello packet
[6:48:01 PM]:3    COM3     5.0724144s     resdump:<?xml version="1.0" encoding="UTF-8" ?>
<data>
<log value="ERROR: Only nop and sig tag can be recevied before authentication." /></data><?xml version="1.0" encoding="UTF-8" ?>
<data>
<response value="NAK" rawmode="false" /></data>


[6:48:26 PM]:3    COM3     30.0507034s     authentication failed result by Ko Nine
[6:50:33 PM]:3    COM3     5.0051592s     resdump:<?xml version="1.0" encoding="UTF-8" ?>
<data>
<log value="ERROR: Only nop and sig tag can be recevied before authentication." /></data><?xml version="1.0" encoding="UTF-8" ?>
<data>
<response value="NAK" rawmode="false" /></data>


[6:50:58 PM]:3    COM3     30.0109683s     authentication failed result by Ko Nine
[6:51:57 PM]:3    COM3     5.0180762s     resdump:<?xml version="1.0" encoding="UTF-8" ?>
<data>
<log value="ERROR: Only nop and sig tag can be recevied before authentication." /></data><?xml version="1.0" encoding="UTF-8" ?>
<data>
<response value="NAK" rawmode="false" /></data>


[6:52:42 PM]:3    COM3     50.0467423s     authentication failed result by Ko Nine AQAAAG0BAABN2o7Pba52vQWYJBc7EjrAJBvjcQ
[7:00:02 PM]:3    COM3     5.000809s     resdump:<?xml version="1.0" encoding="UTF-8" ?>
<data>
<log value="ERROR: Only nop and sig tag can be recevied before authentication." /></data><?xml version="1.0" encoding="UTF-8" ?>
<data>
<response value="NAK" rawmode="false" /></data>


[7:14:57 PM]:3    COM3     900.0314714s     authentication failed result by Ko Nine AQAAAG0BAABN2o7PL3KFD0lhZ9kk1eRFRxgd0A
[7:32:28 PM]:3    COM3     5.0073073s     resdump:<?xml version="1.0" encoding="UTF-8" ?>
<data>
<log value="ERROR: Only nop and sig tag can be recevied before authentication." /></data><?xml version="1.0" encoding="UTF-8" ?>
<data>
<response value="NAK" rawmode="false" /></data>


[7:34:43 PM]:3    COM3     140.0288576s     authentication failed result by Ko Nine AQAAAG0BAABN2o7P8tW3KfeCKfWd-tfEQfjSPg
[7:42:30 PM]:3    COM3     4.9990707s     resdump:<?xml version="1.0" encoding="UTF-8" ?>
<data>
<log value="ERROR: Only nop and sig tag can be recevied before authentication." /></data><?xml version="1.0" encoding="UTF-8" ?>
<data>
<response value="NAK" rawmode="false" /></data>


[7:42:55 PM]:3    COM3     29.9868516s     The system cannot find the file specified
[7:44:10 PM]:3    COM3     6.7644676s     resdump:<?xml version="1.0" encoding="UTF-8" ?>
<data>
<log value="ERROR: Only nop and sig tag can be recevied before authentication." /></data><?xml version="1.0" encoding="UTF-8" ?>
<data>
<response value="NAK" rawmode="false" /></data>


[7:44:55 PM]:3    COM3     51.769318s     Input string was not in a correct format.
[7:47:26 PM]:3    COM3     4.9975509s     resdump:<?xml version="1.0" encoding="UTF-8" ?>
<data>
<log value="ERROR: Only nop and sig tag can be recevied before authentication." /></data><?xml version="1.0" encoding="UTF-8" ?>
<data>
<response value="NAK" rawmode="false" /></data>


[7:48:56 PM]:3    COM3     95.036973s     flash done
[8:11:58 PM]:3    COM3     5.0098869s     resdump:<?xml version="1.0" encoding="UTF-8" ?>
<data>
<log value="ERROR: Only nop and sig tag can be recevied before authentication." /></data><?xml version="1.0" encoding="UTF-8" ?>
<data>
<response value="NAK" rawmode="false" /></data>


[8:12:18 PM]:3    COM3     25.0604197s     No application is associated with the specified file for this operation
[8:14:43 PM]:3    COM3     5.0063974s     resdump:<?xml version="1.0" encoding="UTF-8" ?>
<data>
<log value="ERROR: Only nop and sig tag can be recevied before authentication." /></data><?xml version="1.0" encoding="UTF-8" ?>
<data>
<response value="NAK" rawmode="false" /></data>


[8:16:23 PM]:3    COM3     105.2005221s     resdump:<?xml version="1.0" encoding="UTF-8" ?>
<data>
<log value="ERROR: Signature Verification Failed." /></data><?xml version="1.0" encoding="UTF-8" ?>
<data>
<response value="NAK" rawmode="false" /></data>


[8:20:46 PM]:3    COM3     4.986848s     resdump:<?xml version="1.0" encoding="UTF-8" ?>
<data>
<log value="ERROR: Only nop and sig tag can be recevied before authentication." /></data><?xml version="1.0" encoding="UTF-8" ?>
<data>
<response value="NAK" rawmode="false" /></data>


[8:22:26 PM]:3    COM3     105.1126102s     Input string was not in a correct format.
